|  |  |
| --- | --- |
| Model | WH-B6B-CAM-4G |
| Image Sensor | 3518E  1/3 " illumination CMOS sensor; |
| Effective Pixels | 1280X720P,1280X960P,1920X1080P |
| Pixel | 1.0/1.3/2.0MP |
| Signal System | PAL/NTSC |
| Video Format | 1080P(50HZ), 25fps(60HZ);(960P 25fps(50HZ), 25fps(60HZ);720P 25fps(50HZ), 30fps(60HZ) |
| Min Illumination | Colour 0.01Lux  F1.2, black and white 0.001 Lux F1.2 |
| White Balance | Auto/Manual/ATW/Indoor/Outdoor/Daylight lamp/Sodium lamp |
| AGC | Auto/Manual |
| S/N Ration | >52db |
| BLC | ON/OFF |
| HLC | Support |
| 3D DNR | Support |
| Smart defog | Support |
| DWDR | Support |
| Shutter Time | 1 ~1/1000s |
| Day/Night | ICR |
| Frame Rate | 25fps |
| Privacy Masking | Support 4 rectangle areas |
| Bit Rate | 307Kbps~8Mbps |
| Auto Focus | Auto/Semi-automatic/Manual |
| Optical Zoom | 4X |
| Digital Zoom | 3X |
| Focal Length | 2.8~12mm,4X |
| Zoom Speed | Approx. 3s |
| Angle of View | 91°-28° |
| Minimum Working Distance | 10-600mm |
| Aperture Range | Fix |
| Pan Range | 0°~355°; |
| Pan Speed | Pan Manual Speed: 0.1° ~40°/s, Pan Preset Speed: 40°/s |
| Tilt Range | 0~90° |
| Tilt Speed | Tilt Manual Speed: 0.1° ~40°/s, Tilt Preset Speed: 40°/s |
| Number of pre-set | 128 |
| Patrol | 8 patrols,8 pre-sets per patrol |
| Power loss recovery | Support |
| Park Action | Preset/Patrol/Pattern/Pan Scan |
| Audio Input | Optional(Not Build-In) |
| Audio Output | Optional(Not Build-In) |
| Infrared Lamp | 6pcs 14 Lattice Lamps |
| IR distance | 40m~60m |
| Wavelength | 850nm |
| WIFI | SUPPORT/802.11b/g/n |
| WIFI Distance | 30M |
| Storage | Max support 128G TF card(128G/64G /32G /16G Optional) |
| USIM/SIM | Micro SIM card |
| Wi-Fi Standard | 802.11b/g/n, Max 72Mbps |
| Wi-Fi Frequency | 2412MHz-2472MHz |
| Wi-Fi Safe Mode | Open, WPA-PSK, WPA2-PSK |
| Network type | FDD-LTE, TDD-LTE, WCDMA/HSPA+, TD-SCDMA, GSM/GPRS/EDGE |
| Working  Frequency | LTE B1/B3/B8/B38/B39/B40/B41 |
| WCDMA 2100/900MHz,TD-SCDMA B34/B39 |
| TD-SCDMA B34/B39 |
| GSM/GPRS/EDGE: 900/ 1800MHz |
| Ethernet | 1 RJ45 & Antenna 10M/100M Adaptive Ethernet Interface, 10Base-T/100Base-TX |
| Max. Image Resolution | 1280\*960 |
| Frame Rate | 50Hz: 25 fps (1280×960) , 25 fps (1280×720) |
| 60Hz: 30 fps (1280×960) , 30 fps (1280×720) |
| Main Stream | 50Hz: 25 fps (1280×960) , 25 fps (1280×720) |
| 60Hz: 30 fps (1280×960) , 30 fps (1280×720) |
| Sub Stream | 720P(640x480&640x352),720P(320x240&320x176) |
| JPG rate | Q720P(640x352),QQ720P(320x176) |
| Image Compression | H.264/MJPEG/32Kbps-6144bps |
| Audio Compression | G.711/G.722/G.726/MP2L2(Optional) |
| Protocol | TCP/IP,HTTP,TCP,ICMP,UDP,ARP,IGMP,SMTP,FTP,DHCP,DNS,DDNS,NTP,UPNP,RTSP |
| No. of Simultaneous Users: | Up to 5 users, Three level authority: |
| Administrator/User/Visitor |
| Dual Stream | Support |
| ONVIF | 2.1 |
| Security Measures | User authentication (ID and PW), |
| Host authentication (MAC address) |
| IP address filtering |
| Transmission | Internal Cloudsee Protocol |
| Browser | IE8+,Chrome18+,Firefox5.0+,Safari5.02+ browsers |
| Menu Language | English &Chinese |
| Power Supply | DC 12V 2A |
| Power consumption | Day:<12W Night:<24W |
| Temperature | -20degree~+60degree (-4°F ~ 140°F) |
| Working Humidity | <95% |
| Protection Level | IP66 Standard(outdoor dome) |
| Material | Aluminium |
| Dimensions | 137×228mm (Ceiling) |
| 137×239mm (Wall) |
| G. Weight(kg) | 1.8kg |